Preliminary remark:

PE-HD cable protection pipes according to DIN 16874, with fine or rough longitudinal inner grooves or smooth without grooves or special inner coating. Suitable for direct buried installations, or for insertion in empty conduits, cable-conduits.

Design: Solid wall- or coextruded pipes.

Material: according to DIN 16874

Pipe system monitored by SKZ

Manufacturer certified according to DIN EN ISO 9001, DIN EN ISO 50001, DIN EN ISO 14001

The production of all necessary pipe-connectors is done in accordance with valid technical requirements. The pipes have to be stored and transported to the construction site in accordance with KRV guidelines.

Product: egeplast ege-com® Macroduct Mono

or equivalent

Manufacturer: egeplast international GmbH

Robert-Bosch-Str. 7

D-48268 Greven

Tel.: +49.2575.9710-0

Fax: +49.2575.9710-110

e-mail: info@egeplast.de

http://www.egeplast.de

Specification: egeplast ege-com® Macroduct Mono

Dimension \_\_\_\_\_\_\_\_mm, SDR \_\_\_\_\_

Delivered as straight lengths 6 / 12 m

Delivered as coils with a length of \_\_\_\_\_\_m

Delivered as drums with a length of \_\_\_\_\_\_m.

\_\_\_\_\_\_\_\_\_\_\_m to be delivered and installed professionally, according to DIN and relevant installation guidelines: \_\_\_\_\_\_\_\_\_\_\_\_€/m