****

**RFP form egeModul PE**

Preliminary remark:

Short polyethylene pipes made of PE 80, in accordance with 8074/75, egeplast system, dimensions in accordance with DIN 8074; pipe colour black, at least 2/3 of the wall thickness, with bright, inspection-friendly inner layer.

The short pipes are made with 3-lip seal and longitudinal positive-locking plug-in connectors integrated in the pipe wall. The seal must comply with DIN EN 681-1. The certificate for tests in accordance with DIN EN 1277 must confirm the raised

level of pressure resistance of 2.5 bar with a 3° bend in the socket. A dimension record must be submitted on the manufacture of the milled socket and milled spigot.

Brand: egeplast egeModul PE or equivalent

Manufacturer: egeplast international GmbH

 Robert-Bosch-Str. 7

 D-48268 Greven

 Tel.: +49.2575.9710-0

 Fax: +49.2575.9710-110

 info@egeplast.de

 <http://www.egeplast.eu>

Specifications:

egeplast egeModul PE made of PE-HD in the dimensions:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_mm, SDR\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Length: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_m

Rehabilitation route: \_\_\_\_\_\_\_\_m

Supply \_\_\_\_\_\_\_\_\_\_\_\_\_\_ units and insert professionally in the cleaned and prepared old pipes, including provision of personnel and use of all necessary equipment and machinery including the delivery oft he pipes: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ €/unit