egeLogoneu schwarz(Bitmap).tif

**RFP form egeModul PP**

Preliminary remark:  
Short pipes made of PP-HM, egeplast system, following DIN 8077 and DIN EN

1852; pipe colour black, at least 2/3 of the wall thickness. With bright, inspection-

friendly inner layer.

The short pipes are made with 3-lip seal and axially force-locked socket integrated

in the pipe wall. The seal must comply with DIN EN 681-1. The certificate for

tests in accordance with DIN EN 1277 must confirm the higher level of pressure

resistance of 2.5 bar with a 3° bend in the sleeve. A dimension record must be

submitted on the manufacture of the milled socket and milled spigot.

Brand: egeplast egeModul PP or similar

Manufacturer: egeplast international GmbH

Robert-Bosch-Str. 7

D-48268 Greven

Tel.: +49.2575.9710-0

Fax: +49.2575.9710-110

[info@egeplast.de](mailto:info@egeplast.de)

<http://www.egeplast.>eu

Specifications:

egeplast egeModul PP made of PP-HM in the dimensions of:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_mm, SDR\_\_\_\_\_\_\_\_\_\_\_\_

Length \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_m

Rehabilitation route \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_m

Supply \_\_\_\_\_\_\_\_\_ units and insert professionally in the cleaned and prepared old pipes, including provision of personnel and use of all necessary equipment and machinery including the delivery oft he pipes: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_€/unit